	S/NO
	DESCRIPTION
	QUANTITY
	UNIT
	RATE (N)
	AMOUNT (N)

	1
	PRELIMINARIES
Site clearing/mobilization to site
	I/sum
	
	
	

	2
	Excavation
	I/sum
	
	
	

	
	SUB-STRUCTURE/ SUPER STRUCTURE
﻿
	
	
	
	

	
	Aggregate, sand cement mixture 1:24
	
	
	
	

	1
	Granite
	3
	tons
	
	

	2
	Sharp Sand for laying of blocks
	5
	tons
	
	

	3
	Cement for laying of block/plaster
	30
	bags
	
	

	4
	water/ storage tank
	p/sum
	
	
	

	5
	Blocks
	500
	No.
	
	

	6
	galvanize iron pole 3"
	4
	pcs
	
	

	7
	plaster sand
	5
	tons
	
	

	8
	Sharp Sand for flooring
	3
	tons
	
	

	9
	Cement for floor
	5
	bags
	
	

	10
	Provide hand rail support for ramp entrance
	p/sum
	
	
	

	
	ROOFING
	
	
	
	

	1
	wood 50mmx150mm
	20
	pcs
	
	

	2
	50mmx100mm
	20
	pcs
	
	

	3
	[bookmark: _GoBack]50mmx75mm
	20
	pcs
	
	

	4
	50mmx50mm for noggin
	70
	pcs
	
	

	5
	Ceiling board
	16
	pcs
	
	

	6
	Batting
	1
	roll
	
	

	7
	Nail 5", 4'3'2'
	40
	kg
	
	

	8
	Zink
	3
	bundle
	
	

	9
	zink nail
	8
	kg
	
	

	10
	1x12 plank for facial board
	8
	No.
	
	

	11
	quarter rod for the tie beam
	4
	pcs
	
	

	
	PAINT
	
	
	
	

	1
	White emotion paint 
	20
	Ltrs
	
	

	2
	Orange emotion paint
	20
	Ltrs
	
	

	3
	Oil paint white
	8
	Ltrs
	
	

	
	LABOUR
	
	
	
	

	1
	Labour for Carpenter
	I/sum
	
	
	

	2
	Labour for Mason
	I/sum
	
	
	

	3
	Labour for Painter
	I/sum
	
	
	

	4
	Labour for Welder
	I/sum
	
	
	

	5
	Transporting materials to site
	P/sum
	
	
	

	
	sub -total
	
	
	
	

	
	Contingency
	
	
	5%
	

	
	Sub- Total
	
	
	
	

	
	
	
	
	
	

	
	GRAND TOTAL
	
	
	
	



